## Mirrors

#### Mirror Holder Replacement

20-5

1. Carefully pull out the bottom edge of the mirror holder (A) by hand. Take care not to scratch the mirror.

2. Separate the mirror holder from the actuator (B) by slowly pulling them apart while detaching the clips (C). If equipped, disconnect the mirror defogger connectors (D) from the heater pad terminals.
3. If equipped, reconnect the mirror defogger connector.
4. Reattach the clips of the mirror holder to the actuator, then position the mirror holder on the actuator. Carefully push on the clip portions of the mirror holder until the mirror holder locks into place.
5. Check the operation of the actuator.