## Transmission End Cover

#### End Cover, 1st Gears and 1st Clutch Removal (cont'd)

14-173

Special Tools Required Mainshaft holder set, 07PAB-0010000 NOTE: Refer to the Exploded View as needed during the following procedure.

1. Remove the transmission range switch cover.
2. Remove the transmission range switch harness clamps, then remove the transmission range switch.
3. Remove the 12 bolts securing the end cover, then remove the end cover.
4. Slip the special tool onto the mainshaft.

5. Engage the park pawl with the park gear.
6. Cut the lock tabs (A) of the mainshaft and countershaft locknuts (B) using a chisel (C). Then remove the locknuts and conical spring washers from both shafts.

NOTE:

- Mainshaft and countershaft locknuts have left-hand threads.
- Clean the old countershaft locknut; it is used to install the press fit park gear on the countershaft.
- Keep all of the chiselled particles out of the transmission.

7. Remove the special tool from the mainshaft.

8. Remove the 1st clutch and mainshaft 1st gear as an assembly and remove the 1st gear collar.
9. Remove the park pawl, park pawl spring, park pawl shaft and stop shaft.
10. Remove the park lever from the control shaft.
11. Remove the park gear, one-way clutch and countershaft 1st gear assembly (A) using a universal 2 jaw puller (B).

12. Remove the needle bearing and countershaft 1st gear collar.
13. Remove the ATF cooler lines.
14. Remove the A/T clutch pressure control solenoid valves A and B, if necessary.