## Maintenance Schedule for Severe Conditions

#### (European Model) (cont'd)

3-7

NOTES | SECTION and PAGE
| (see page 8-5)
| (see page 8-6)
| (see page 11-147) (see page 11-447)
Check the valve clearance. | (see page 6-14)
| (see page 11-138) (see page 11-296) (see page 11-438) (see page 11-571)
| (see page 4-25)
Check water pump for signs of seal leakage. | (see page 6-18) (see page 6-22) (see page 10-7)

- Check for cracks and damage.
- Check deflection and tension.

(see page 17-23)
| (see page 11-125) (see page 11-285) (see page 11-425) (see page 11-560)
Check specific gravity for freezing point. | (see page 10-8)
Use genuine Honda MTF (Manual Transmission Fluid). | (see page 13-3)
Use genuine Honda AFT-Z1 (ATF). | (see page 14-122)

- Check the brake pad and disc thickness. Check for damage or cracks.
- Check the wheel cylinder for leaks.
- Check the brake linings for cracking, glazing, wear or contamination.
- Check the calipers for damage, leaks and tightness.

(see page 19-3)
Use only DOT 3 brake fluid. (We recommend Genuine Honda Brake Fluid.) Check that Brake fluid level is between the upper and lower marks on the reservoir. | (see page 19-7)
Check the parking brake operation. | (see page 19-6)
| -
Check the position of the headlight. | (see page 22-144)
Check for road stability, noise, vibrations and dashboard operation. | -

- Check for correct installation and position, check for cracks, deterioration rust and leaks.
- Check tightness of screws, nuts and joints. If necessary, retighten.

-

- Check rack grease and steering linkage. Check the boot for damage and leaking grease.
- Check the fluid line for damage and leaks.

(see page 17-5)

- Check the bolts for tightness.
- Check all dust covers for deterioration and damage.

(see page 18-3)

- Check the boot and boot band for cracks
- Check rack grease.

(see page 16-3)
Check the master cylinder, proportioning control valve and ABS modulator and leakage. | (see page 19-48)
Check for leaks. | -
Check the catalytic converter heat shield, exhaust pipe and muffler for damage, leaks and tightness. | (see page 9-5)
Check fuel lines for loose connections, cracks and deterioration. Retighten loose connections and replace any damaged parts | (see page 11-132) (see page 11-290) (see page 14-232) (see page 11-565)
Check for pressure, puncture or cuts and irregular tread wear. | -

NOTE: If the customer's vehicle is driven OCCASIONALLY under severe condition, you should follow the Normal Condition Maintenance Schedule on pages 3-4 and 3-5.