## Power Steering

#### Steering Gearbox Removal (cont'd)

17-38

18. Lower the steering gearbox, and rotate it so the pinion shaft points upward.

19. Carefully move the steering gearbox (A) and tie-rods (B) as an assembly toward the passenger's side until the pinion shaft clears the heater hoses. Remove the steering gearbox through the wheel well opening on the passenger's side.

20. Remove the pinion shaft grommet (C) from the top of the valve body unit.