## Design Specifications

#### (cont'd)

2-18

Item | Measurement | Qualification | Specification
ENGINE | Type | D17A2, D17A5, D17A9 engines | Water-cooled, 4-stroke SOHC VTEC engine
D17A8 engine | Water-cooled, 4-stroke SOHC engine
Cylinder arrangement |  | Inline 4-cylinder, transverse
Bore and stroke |  | 75 x 94.4 mm (2.95 x 3.72 in.)
Displacement |  | 1,668 cm3 (102 cu in.)
Compression ratio | D17A8, D17A5 engines | 9.5
D17A2, D17A9 engines | 9.9
Valve train | D17A2, D17A5, D17A9 engines | Belt driven, SOHC VTEC 4 valves per cylinder
D17A8 engine | Belt driven, SOHC 4 valves per cylinder