## Automatic Transmission

#### System description (cont'd)

14-56

Hydraulic Flow (cont'd)

Position

The PCM turns the shift solenoid valve A and B OFF. Line pressure (1) passes through the manual valve, but it does not flow to the clutches. Line pressure (1) also flows to the modulator valve and becomes to modulator pressure (6). Modulator pressure (6) flows to the shift valves by means of the shift solenoid valves A and B OFF.

Under this condition, hydraulic pressure is not applied to the clutches.

NOTE:

- When used, ''left'' or ''right'' indicates direction on the hydraulic circuit.
- There are 4 hydraulic circuits; 6-position, 6-position with the 3rd sub accumulator, 7-position and 7-position with the 3rd sub accumulator. The illustration shows the 7-position transmission circuit; 6-position circuit does not include 1st-hold clutch line.