## Keyless/Power Door Lock System

#### Super Locking Control Unit Input Test (cont'd)

22-235

Cavity | Wire | Test condition | Test: Desired result | Possible cause if result is not obtained
3 | BLK | Under all conditions | Check for continuity to ground: There should be continuity. |

- Poor ground (G501, G502, G551)
- An open in the wire

2 | YEL/BLK | Connect the No. 2 terminal to the No. 7 terminal and the No. 6 terminal to the No. 3 terminal momentarily with ignition switch ON (II) | Check actuator operation: The actuator should lock. |

- Faulty door lock actuator
- An open in the wire

7 | LT GRN [GRY]
5 | YEL | Connect the No. 5 terminal to the No. 6 terminal and the No. 7 terminal to the No. 3 terminal momentarily with ignition switch ON (II) | Check actuator operation: The actuator should unlock.
6 | LT GRN/RED [GRY/BLU]
4 | LT GRN/BLK [GRY/RED] | Under all condition | Check for continuity between the No. 4 terminal and No. 7 terminal of the actuator. There should be continuity. |

- An open in the wire

[ ]: Passenger's