## Rear Side Outer Panel

#### Removal

3-27

- Cut and pry off rear side outer panel.
- Check the rear combination adaptor position for damage and if necessary, replace the rear combination adopter and rear gutter as an assembly.

  1. REAR INNER PANEL
  2. REAR DAMPER STIFFENER
  3. PARCEL SHELF
  4. INNER PANEL EXTENSION
  5. REAR FLOOR
  6. REAR GUTTER
  7. REAR PANEL
  8. REAR COMBINATION ADAPTOR
  9. OUTER PANEL