## Manual Transmission

#### Transmission Disassembly

13-16

Exploded View-Clutch Housing

1 2 3 4 5

6

7

8

9

10

11

DIFFERENTIAL ASSEMBLY

SHIFT FORK ASSEMBLY

6mm FLANGE BOLT

(12 Nm (1.2 kgf/m, 9 lbf/ft)

BEARING SET PLATE

COUNTERSHAFT ASSEMBLY

NEEDLE BEARING

OIL GUIDE PLATE C

14 x 20 mm DOWEL PIN

MAGNET

MAINSHAFT ASSEMBLY

28 mm WASHER

12

13

14

15

16

17

18

19

28 mm SPRING WASHER

BALL BEARING

28 x 43 x 7 mm OIL SEAL

Replace.

REVERSE GEAR SHAFT

REVERSE IDLER GEAR

6 mm SPECIAL BOLT

15 Nm (1.5 kgf/m, 11 lbf/ft)

REVERSE SHIFT FORK

35 x 58 x 8 mm OIL SEAL

Replace.

20

21

22

23

24

25

26

BACK-UP LIGHT SWITCH

29 Nm (3.0 kgf/m, 22 lbf/ft)

O-RING

Replace.

VEHICLE SPEED SENSOR (VSS)

8 mm FLANGE BOLT

22 Nm (2.2 kgf/m, 16 lbf/ft)

CLUTCH HOUSING

TRANSMISSION HANGER

10 mm FLANGE BOLT

44 Nm (4.5 kgf/m, 33 lbf/ft)

a a a