## Heating

#### Symptom Troubleshooting Index (cont'd)

21-10

5-door Except KE Model

Symptom | Diagnostic procedure | Also check for
Recirculation control doors do not change between Fresh and Recirculate. | Recirculation Control Motor Circuit Troubleshooting (see page 21-37) |

- Blown fuse No. 14 (10A) in the under-dash fuse/relay box
- Cleanliness and tightness of all connectors

Blower motor runs, but one or more speeds are inoperative. | Blower Motor Circuit Troubleshooting (see page 21-39) |

- Cleanliness and tightness of all connectors

Blower motor does not run at all. | Blower Motor Circuit Troubleshooting (see page 21-39) |

- Blown fuse No. 12 (40A) in the under-hood fuse/relay box and No. 14 (10A) in the under-dash fuse/relay box
- Poor ground at G201 and G501
- Cleanliness and tightness of all connectors