## Intake Air System

#### Throttle Body Removal/Installation

11-129

NOTE:

- Do not adjust the throttle stop screw.
- After reassembly, adjust the throttle cable (see page 11-127).
- The Throttle Position (TP) sensor is not removable.

1. THROTTLE STOP SCREW

   (Do not adjust)

2. THROTTLE LEVEL
3. There should be no clearance
4. MANIFOLD ABSOLUTE PRESSURE (MAP) SENSOR
5. THROTTLE CABLE
6. IDLE AIR CONTROL (IAC) VALVE
7. THROTTLE POSITION (TP) SENSOR
8. EVAPORATIVE EMISSION (EVAP) CANISTER PURGE VALVE
9. GASKET, Replace.

a a a