## Manual Transmission

#### Change Lever Assembly Disassembly/Reassembly

13-22

NOTE:

- Prior to reassembling, clean all the parts in solvent, dry them and apply lubricate to any contact surface.
- If 5 minutes have passed after applying liquid gasket, reapply it and assemble the shift arm cover.

1. SHIFT LOCK CAM A
2. ROLLER
3. SHIFT ARM COVER
4. BREATHER CAP

   Turn the arrow toward the front of the vehicle, and install it.

5. DUST SEAL, Replace.
6. SELECT LEVER

   Be careful not to damage the dust seal when installing it.

7. DUST COVER
8. SHIFT LEVER
9. WASHER
10. OIL SEAL, Replace.
11. 1ST/2ND SELECT SPRING
12. INTERLOCK
13. SHIFT ARM
14. 8 mm SPRING WASHER
15. 8 mm SPECIAL BOLT

    31 Nm (3.2 kgf/m, 23 lbf/ft)

16. MBS RETURN SPRING
17. MBS ARM
18. 5TH SELECT SPRING
19. SELECT STOP PLATE
20. SCREW, Replace.
21. Stake
22. REVERSE LOCKOUT SOLENOID

    Apply liquid gasket (P/N 08C70-K0234M) to the sealing surface.

23. BREATHER PLATE

a a a