## Keyless/Power Door Lock System

#### Keyless Receiver Unit Input Test

22-226

1. Remove the dashboard centre lower cover (see page 20-79).
2. Remove the audio unit (see page 22-212).
3. Disconnect the 5P connector (A) from the keyless receiver unit (B).

Wire side of female terminals

4. Inspect the connector and socket terminals to be sure they are all making good contact.

- If the terminals are bent, loose or corroded, repair them as necessary and recheck the system.
- If the terminals are OK, go to step 5.