## Seat Belts

#### Front Seat Belt Replacement (cont'd)

23-6

8. Remove the centre pillar upper trim (see page 20-64).

9. Remove the shoulder anchor adjuster (A).

10. Install the seat belt in the reverse order of removal and note these items:

- Apply liquid thread lock to the upper anchor bolt before reinstallation.
- Check that the retractor locking mechanism functions (see page 23-11).
- Assemble the washers, collar and bushing on the upper and lower anchor bolts as shown.
- Before installing the anchor bolts, make sure there are no twists or kinks in the front seat belt.
- If equipped, make sure the seat belt tensioner connector is plugged in properly.
- If equipped with a seat belt tensioner, reconnect the negative cable to the battery.
- If equipped, enter the anti-theft code for the radio, then enter the customer's radio station presets.

Upper anchor bolt construction:

1. COLLAR
2. UPPER ANCHOR
3. UPPER ANCHOR BOLT
4. BUSHING
5. TOOTHED LOCK WASHER

Lower anchor bolt construction:

1. COLLAR
2. WASHER
3. COLLAR
4. LOWER ANCHOR BOLT
5. BUSHING
6. LOWER ANCHOR
7. SPRING WASHER
8. TOOTHED LOCK WASHER