## Body

####

Doors

Component Location Index - Front Door | 20-2
Front Door Panel Removal/Installation - Manual Window | 20-3

Mirrors

Mirror Holder Replacement | 20-5

Interior Trim

*Carpet Replacement | 20-6

Bumpers

Front Bumper Removal/Installation | 20-8

Tailgate

Tailgate Support Strut Replacement | 20-9

Exterior Trim

Emblem Replacement | 20-10

Openers

Hood Opener Cable Replacement | 20-11
Fuel Fill Door Opener Cable Replacement | 20-12

NOTE: Refer to the '01 Civic Shop Manual, P/N 62S5A00 on this CD, for the items not shown in this manual.

Outline of 5-door Model Changes

- The U.K. Manufacturing produced vehicles have been added. The LHD models have been added; the LHD models are symmetrical and same manner against the RHD models.

- On the front door for some models, the manual windows have been added.
- For some models, the manual door mirror has been added; the mirror holder removal/installation procedures are different.
- The footrest removal/installation procedures are different.
- For some models the headlight washer has been equipped to the front bumper.
- The tailgate support strut replacement procedure is different.
- Some emblems have been added and the attachment points are different.
- For the LHD models, the hood and fuel fill door opener cables replacement procedures have been added.

This model has an SRS which includes a driver's airbag in the steering wheel hub, a passenger's airbag in the dashboard above the glove box, seat belt tensioners in the front seat belt retractors and some models include side airbags in the front seat-backs. Information necessary to safely service the SRS is included in the Shop Manual P/N 62S5A00 on this CD. Items marked with an asterisk (*) on the contents page include or are located near, SRS components. Servicing, disassembling or replacing these items will require special precautions and tools and should be done only by an authorised Honda dealer.

WARNING

- To avoid rendering the SRS inoperative, which could lead to personal injury or death in the event of a severe frontal collision, all SRS service work must be performed by an authorised Honda dealer.
- Improper service procedures, including incorrect removal and installation of the SRS, could lead to personal injury caused by unintentional deployment of the airbags.
- Do not bump the SRS unit. Otherwise, the system may fail in a collision, or airbags may deploy when the ignition switch is ON (II).
- SRS electrical wiring connectors are identified by yellow colour coding. Related components are located in the steering column, front console, dashboard, dashboard lower panel and in the dashboard above the glove box. Do not use electrical test equipment on these circuits.