## Transmission Housing/Flywheel Housing

#### Driven Pulley Shaft Bearing Removal/Installation

14-359

Special Tools Required

- Snap ring pliers, 07LGC-0010100
- Handle driver, 07749-0010000
- Driver attachment, 72 x 75 mm, 07746-0010600

NOTE: Coat all parts with ATF before assembly.

1. To remove the driven pulley shaft bearing from the transmission housing, expand the snap ring with the special tool, then push the bearing out.

   NOTE: Do not remove the snap ring unless it's necessary to clean the groove in the housing.

2. Install the bearing (A) in the direction shown.

3. Expand the snap ring with the special tool and install the bearing part-way into the housing.
4. Release the pliers, then push the bearing down into the housing until the snap ring snaps in place around it.
5. After installing the bearing verify that the snap ring (A) is seated in the bearing and housing grooves and that the ring end gap (B) is correct.