## Front Suspension

#### Stabiliser Link Replacement (cont'd)

18-18

1. Raise the front of the vehicle and make sure it is securely supported. Remove the front wheels.

2. Remove the self-locking nut (A) and flange nut (B) while holding the respective joint pin (C) with a hex wrench (D) and remove the stabiliser link (E).

3. Install the stabiliser link on the stabiliser bar and lower arm with the joint pins set at the centre of each moving range.

4. Install the self-locking nut and flange nut and lightly tighten them.

NOTE: Use a new self-locking nut on reassembly.

5. Place the floor jack under the lower arm ball joint and raise the suspension to load it with the vehicle's weight.

Do not place the jack against the flat section of the lower arm. Lifting the arm in this area might bend it.

6. Tighten the self-locking nut (A) and flange nut (B) to the specified torque values while holding the respective joint pins (C) with a hex wrench (D).

7. After 5 minutes, re-tighten the self-locking nut again with the specified torque.