## General Information

#### Exterior Parts Removal/Installation

1-20

NOTE: To adjust the alignment of the hood, the front door, rear door and trunk lid, refer to the CIVIC Shop Manual.

Mounting bolts/nuts torque:

6X1.0 mm: 9.8 Nm (1.0 kgf/m, 7.2 lbf/ft)

*6X1.0 mm: 1.8 Nm (1.8 kgf/m, 13 lbf/ft)

8X1.0 mm: 22 Nm (2.2 kgf/m, 16 lbf/ft)

*8X1.25 mm: 29 Nm (3.0 kgf/m, 22 lbf/ft)

1. HOOD
2. HOOD HINGE
3. REAR BUMPER SIDE BRACKET
4. TAILGATE HINGE
5. TAILGATE
6. REAR BUMPER BEAM
7. FUEL DOOR
8. REAR BULKHEAD GUSSET
9. REAR DOOR
10. REAR DOOR HINGE
11. FRONT DOOR
12. FRONT DOOR HINGE
13. FRONT FENDER
14. CORNER UPPER BEAM
15. FRONT BUMPER BEAM
16. FRONT BUMPER LOWER STIFFENER
17. BATTERY SET BASE