## Side Sill Outer Panel

#### Removal

3-3

- Cut and pry off the side sill outer panel.
- Check the centre pillar stiffener and side sill reinforcement position and check for damage. If necessary replace the side sill reinforcement.
- Replace the driver's side sill reinforcement as an assembly because of the way the stiffener is attached inside the side sill reinforcement.

  1. OUTER PANEL
  2. SIDE SILL REINFORCEMENT
  3. REINFORCEMENT STIFFENER (Driver side)
  4. INSIDE SILL
  5. REAR INNER PANEL
  6. SIDE SILL REINFORCEMENT
  7. VIEW (Z)
  8. CENTRE PILLAR STIFFENER
  9. OUTER PANEL STIFFENER
  10. WHEEL ARCH EXTENSION
  11. SIDE SILL REINFORCEMENT
  12. OUTER PANEL
  13. FRONT PILLAR LOWER STIFFENER