## Dashboard

#### Dashboard Centre Lower Cover Removal/Installation

20-217

NOTE:

- When prying with a flat-tip screwdriver, wrap it with protective tape and apply protective tape around the related parts, to prevent damage.
- Take care not to scratch the dashboard and related parts.

1. Remove the ashtray holder (A).

1. Remove the ashtray (B).
2. Remove the screws, then remove the ashtray holder.
3. Disconnect the ashtray light bulb socket (C).

Fastener Locations
: Screw, 3

2. Remove the dashboard centre lower cover (A).

1. Remove the screws (B) and clips (C).
2. Gently pull out the cover to release the hooks (D) and pins (E).

   Fastener Locations
   B : Screw, 2 | C : Clip, 2

3. Install the cover in the reverse order of removal and note these items:

- Replace any damaged clips.
- Make sure the ashtray light bulb socket is connected properly.