## Standards and Service Limits

#### Cooling

2-8

Item | Measurement | Qualification | Standard or New | Service Limit
Radiator | Coolant capacity (Includes engine, heater, hoses and reservoir) | M/T: engine overhaul | 5.1 l (5.4 US qt, 4.5 Imp qt)
M/T: coolant change | 4.0 l (4.2 US qt, 3.5 Imp qt)
A/T, HONDA MULTI MATIC: engine overhaul | 5.0 l (5.3 US qt, 4.4 Imp qt)
A/T, HONDA MULTI MATIC: coolant change | 3.9 l (4.1 US qt, 3.4 Imp qt)
Reservoir | Coolant capacity |  | 0.4 l (0.4 US qt, 0.4 Imp qt)
Radiator cap | Opening pressure |  | 93-123 kPa (0.95-1.25 kgf/cm2, 14-18 psi)
Thermostat | Opening temperature | Begin to open | 76-80°C (169-176°F)
Fully open | 90°C (194°F)
Valve lift at fully open |  | 8.0 mm (0.31 in.) min.
Radiator fan switch | Thermoswitch "ON" temperature |  | 91-95°C (196-203°F)
Thermoswitch "OFF" temperature |  | Subtract 3-8°C (5-15°F) from actual "ON" temperature