## Security System

#### Door Lock Knob Switch Test (cont'd)

22-263

Driver's door (5-door):

1. Remove the driver's door panel (see page 20-144).
2. Disconnect the 6P connector (A) from the super locking actuator.

Terminal side of male terminals

3. Check for continuity between the terminals.

- There should be continuity between the No. 3 and No. 4 terminals when the door lock knob switch is LOCK position.
- There should be continuity between the No. 1 and No. 4 terminals when the door lock knob switch is UNLOCK position.

Passenger's door (5-door):

1. Remove the passenger's door panel (see page 20-7).
2. Disconnect the 3P connector (A) from the actuator.

Terminal side of male terminals

3. Check for continuity between the terminals.

- There should be continuity between the No. 1 and No. 4 terminals when the door lock knob switch is UNLOCK position.