## SRS

#### DTC Troubleshooting (cont'd)

23-92

8. Disconnect the FSR1i connector (A) from the right front sensor.

9. Disconnect the U1o connector (A) from the SRS unit (B).

10. Check resistance between the No. 1 and No. 12 terminals of the U1o connector. There should be 1 M ohm or more.

U1o CONNECTOR

Wire side of female terminals

Is the resistance as specified?

YES - Go to step 11.

NO - Short in the engine compartment wire harness or dashboard wire harness B; replace the faulty harness.

11. Reconnect the battery negative cable.
12. Turn the ignition switch ON (II).
13. Check the voltage between the No. 1 terminal of the U1o connector and the body ground. There should be 1 V or less.

U1o CONNECTOR

Wire side of female terminals

Is the voltage as specified?

YES - Go to step 14.

NO - Short to power in the engine compartment wire harness or dashboard wire harness B; replace the faulty harness.