## PGM-FI System

#### MIL Circuit Troubleshooting (cont'd)

11-81

1. Remove the PGM-FI main relay 1 (A).

LHD model:

RHD model:

1. Check for continuity between ECM connector terminal E9 and body ground.

ECM CONNECTOR E (31P)

Wire side of female terminals

Is there continuity?

YES - Repair short in the wire between the No. 17 FUEL PUMP (15A) fuse and the ECM (E9), or the No. 17 FUEL PUMP (15 A) fuse and the PGM-FI main relay 2. Also replace the No. 17 FUEL PUMP (15A) fuse.

NO - Go to step 35.

1. Remove the rear seat cushion, refer to the 2001 Civic 3-door Shop Manual (see page 20-40).

1. Remove the access panel from the floor.

1. Disconnect the fuel pump 5P connector.

1. Check for continuity between the fuel pump 5P connector terminal No. 5 and body ground.

FUEL PUMP 5P CONNECTOR

Wire side of female terminals

Is there continuity?

YES - Repair short in the wire between the fuel pump and the PGM-FI main relay 2. Also replace the No. 17 FUEL PUMP (15A) fuse.

NO - Go to step 39.

1. Reinstall the PGM-FI main relay 2 (A).

LHD model:

RHD model:

a a a