## Rear Suspension

#### Damper/Spring Replacement

18-36

Exploded View

1. SELF-LOCKING NUT

   10 x 1.25 mm, 29 Nm (3.0 kgf/m, 22 lbf/ft), Replace.

2. DAMPER MOUNTING COLLAR
3. DAMPER MOUNTING WASHER

   Check for weakness.

4. DUST COVER
5. DAMPER MOUNTING PLATE
6. BUMP STOP COVER

   Check for vending and damage.

7. BUMP STOP PLATE
8. BUMP STOP

   Check for weakness and damage.

9. DAMPER UNIT

   Check for oil leak, gas leak and smooth operation.

10. DAMPER SPRING

    Check for weakened compression and damage.

11. SPRING MOUNTING CUSHION

    Check for deterioration and damage.

12. DAMPER MOUNTING BUSHING
13. DAMPER MOUNTING BASE
14. DAMPER MOUNTING BUSHING