## Dashboard

#### Instrument Panel Removal/Installation

20-75

Driver's Dashboard Under Cover Removal/Installation

NOTE:

- When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage.
- Take care not to scratch the dashboard and related parts.
- LHD is shown, RHD is symmetrical.

1. Tilt the steering column down.
2. Remove the steering column upper cover (see page 17-9).
3. Remove the instrument panel (A).

1. Remove the screws (B).
2. Gently pull out along the bottom to release the clips (C) and hooks (D).
3. Gently pull out the upper portion of the panel.

   Fastener Locations
   B : Screw, 2 | C : Clip, 2

4. Install the panel in the reverse order of removal.

NOTE:

- Take care not to scratch the dashboard and related parts.
- LHD is shown, RHD is symmetrical.

1. Remove the driver's dashboard under cover (A).

1. Adjust the steering column upward.
2. Turn the lock knob (B) 45°.
3. Gently pull down the rear edge to release the clip (C).
4. Pull the cover away to release it from the clip (D).

2. Install the cover in the reverse order of removal.