## SRS

#### DTC Troubleshooting - with Side Airbags (cont'd)

23-95

12. Check resistance between the No. 6 and No. 17 terminals of the U2o connector. There should be 2.0 - 3.0 ohm.

U2o CONNECTOR

Wire side of female terminals

Is the resistance as specified?

YES - Faulty SRS unit or poor contact at the U2o connector and the SRS unit; check the connection at the U2o connector and SRS unit. If the connector is OK, replace the SRS unit.

NO - Open or increased resistance in the floor wire harness; replace the floor wire harness.

DTC 11-3: Short to Another Wire or Decreased Resistance in Driver's Side Airbag Inflator (With OPDS Unit Model)

1. Erase the DTC memory (see page 23-38).
2. Turn the ignition switch ON (II), and check that the SRS indicator light comes on for about 6 seconds and then goes off.

Does the SRS indicator light stay on?

YES - Go to step 3.

NO - Intermittent failure, system is OK at this time. Go to Troubleshooting Intermittent Failures (see page 23-38).

3. Turn the ignition switch OFF. Disconnect the battery negative cable and wait for 3 minutes.
4. Disconnect the SDi connector (A) from the driver's side airbag (B).

5. Connect the special tool (2 ohm) to the SDi connector.
6. Reconnect the battery negative cable.
7. Erase the DTC memory.