## Accurate Inspection of Damaged Parts (Visual)

#### Measurement

2-5

Whenever possible, make judgements and conclusions based on measurements.

- Measure the wheel alignment to prevent uneven tyre wear or incorrect steering wheel alignment.
- If there are any deviations, use a tram-tracking gauge and measure the body parts.

- If there is any twisting to the body, measure with a frame centring gauge.

- To measure body dimensions, use a universal tram gauge and convex tool.

Body Measuring Dimension/Opening Repair Chart:

Frame Repair Chart:

Diagonal measurement: