## SRS

#### DTC Troubleshooting - with Side Airbags (cont'd)

23-116

12. Check resistance between the No. 18 and No. 8 terminals of the U2o connector, and between the No. 18 and No. 9 terminals of the U2o connector. There should be 1 M ohm or more.

U2o CONNECTOR

Wire side of female terminals

Is the resistance as specified?

YES - Faulty SRS unit; replace the SRS unit.

NO - Short to power in the floor wire harness; replace the floor wire harness.

DTC 12-5: Short to Ground in Right Side Airbag Inflator (Without OPDS Unit Model)

1. Erase the DTC memory (see page 23-38).
2. Turn the ignition switch ON (II), and check that the SRS indicator light comes on for about 6 seconds and then goes off.

Does the SRS indicator light stay on?

YES - Go to step 3.

NO - Intermittent failure, system is OK at this time. Go to Troubleshooting Intermittent Failures (see page 23-38).

3. Turn the ignition switch OFF. Disconnect the battery negative cable, and wait for 3 minutes.
4. Disconnect the SRi connector (A) from the right side airbag (B).

5. Connect the special tool (2 ohm) to the SRi connector.