## Doors

#### Front Door Panel Removal/Installation (cont'd)

20-145

4. Disconnect the power window switch connector (A) and remove the screws from the grip base (B) and door panel (C).

Fastener Locations
: Screw, 3

5. Release the clips that hold the door panel (A) with a commercially available trim pad remover (B), then remove the door panel by pulling it upward. Remove the door panel with as little bending as possible to avoid creasing or breaking it.

   Fastener Locations
   : Clip, 7

6. Install the door panel in the reverse order of removal and note these items:

- Replace any damaged clips.
- Make sure the connector is plugged in properly and the rod is connected properly.