## Installation and Inspection

####

2-11

1. Check the clearance of the door, hood, tailgate and adjust if necessary.
   Check the operation of the parts and make sure the doors lock securely.

1. Apply the sealer to the hinges of the hood, door and tailgate.

1. HOOD HINGE
2. DOOR HINGE
3. TAILGATE HINGE

1. Adjust the wheel alignment.
2. Check the windows for water leaks.
3. Clean the passenger compartments.