## Power Distribution

#### Fuse to Components Index

22-6

Under-hood Fuse/Relay Box

Fuse Number | Amps | Wire Colour | Component(s) or Circuit(s) Protected
1 | 20 A | BLU/YEL | Condenser fan motor
BLU/RED | A/C compressor clutch
2 | 15 A | WHT/GRN | Climate control unit, Dash lights, Front parking lights, Front side marker lights, Heater control panel, License plate lights, Taillights
3 | 7.5 A | WHT/BLU | Ceiling light, Spotlights, Trunk light
4 | 20 A | BLU/BLK | Radiator fan motor
5 | 10 A | WHT/BLK | Turn signal/hazard relay, Turn signal lights
6 | 15 A | WHT/BLK | CKP sensor, ECM/PCM, Injectors, IAC valve, Immobiliser control unit-receiver, PGM-FI main relay 1 and 2, TDC sensor
7 | 15 A | WHT/GRN | Horn, Brake lights, Brake signals (to ABS modulator-control unit, Cruise control unit, ECM/PCM, Multiplex control unit)
8 | 20 A | WHT/GRN | ABS modulator unit
9 | 10 A | WHT/RED | Data link connector (DLC), Gauge assembly, Immobiliser control unit-receiver, Keyless receiver unit, Multiplex control unit, Security control unit, Audio unit
10 | 40 A | WHT/RED | ABS modulator unit
11 | 30 A | BLK/YEL | Rear window defogger, Antenna module
12 | 40 A | BLU/WHT | Blower motor
13 | 40 A | WHT/BLK | No. 7 fuse (in the under-dash fuse/relay box), Power window relay
14 | 40 A | WHT/RED | No. 3, and 16 fuses (in the under-dash fuse/relay box)
15 | 15 A | RED/YEL | High beam indicator light, Left headlight
16 | 20 A | WHT | Multiplex control unit
17 | 15 A | RED | Right headlight
18 | - | - | Not used
19 | 80 A | - | Battery, Power distribution
20 | 50 A*1 | WHT | Ignition switch (BAT)
40 A*2

*1: KG, KE, KR

*2: KB, KK, KX, KY

: Spare Fuse