## Cooling System

#### Radiator and Fan Replacement

10-11

1. Drain engine coolant.
2. Remove the front bumper (see page 20-104).
3. Remove the hood latch (see page 20-106).
4. Remove the upper and lower radiator hoses and ATF cooler hoses.

   1. A/C CONDENSER FAN ASSEMBLY
   2. O-RING

      Replace.

   3. UPPER RADIATOR HOSE
   4. RADIATOR CAP
   5. UPPER BRACKET AND CUSHION
   6. RADIATOR
   7. COOLANT RESERVOIR
   8. LOWER RADIATOR HOSE
   9. CONDENSER BRACKET
   10. LOWER CUSHION
   11. FAN MOTOR CONNECTORS
   12. ATF COOLER HOSES
   13. DRAIN PLUG
   14. RADIATOR FAN ASSEMBLY

5. Disconnect the fan motor connectors and compressor clutch connector.
6. Remove the radiator upper brackets, then pull up the radiator.
7. Remove the fan shroud assemblies and other parts from the radiator.
8. Install the radiator in the reverse order of removal. Make sure the upper and lower cushions are set securely.
9. Fill the radiator with engine coolant and bleed the air.