## Rear Floor

#### Installation

3-34

1. Set the new rear cross-member and rear frame B, into position.
2. Check the body dimensions (see section 4).
3. Tack weld the rear cross-member and rear frame B.
4. Set the new rear floor to align it with the body.
   Cut the new rear floor so it overlaps the body side floor by about 40 mm (1.6 in.).

1. NEW REAR FLOOR
2. Overlap

   40 mm (1.6 in.)

3. NEW REAR FLOOR
4. REAR FLOOR CROSS-MEMBER
5. REAR FLOOR

   (body side)

1. Check the position of the rear inner panel and rear panel.
2. Remove the new rear floor and plug weld the rear floor cross-member.
3. Finish plug welding the area, and take not to grind excessively.

1. REAR FLOOR CROSS MEMBER

8. Set the new rear floor, and plug weld the rear floor cross-member, rear frame B and rear frame A.

1. REAR FRAME A
2. REAR FLOOR CROSS-MEMBER
3. REAR FRAME B
4. REAR FRAME A
5. REAR FLOOR CROSS-MEMBER

1. Perform the main welding to the rear floor.

1. Filler welding