## Climate Control

#### DTC Troubleshooting Index (cont'd)

21-106

5-door

DTC (Recirculation Indicator Light Blinks) | Detection Item | Page
1 | An open in the in-car temperature sensor circuit | (see page 21-128)
2 | A short in the in-car temperature sensor circuit | (see page 21-129)
3 | An open in the outside air temperature sensor circuit | (see page 21-129)
4 | A short in the outside air temperature sensor circuit | (see page 21-131)
5 | An open in the sunlight sensor circuit | (see page 21-131)
6 | A short in the sunlight sensor circuit | (see page 21-132)
7 | An open in the air mix control motor circuit | (see page 21-133)
8 | A short in the air mix control motor circuit | (see page 21-133)
9 | A problem in the air mix control linkage, door or motor | (see page 21-134)
10 | An open or short in the mode control motor circuit | (see page 21-135)
11 | A problem in the mode control linkage, doors or motor | (see page 21-136)
12 | A problem in the blower motor circuit | (see page 21-137)
13 | A problem in the EEPROM in the climate control unit; the control unit must be replaced. | (see page 21-153)
14 | An open in the evaporator temperature sensor circuit | (see page 21-140)
15 | A short in the evaporator temperature sensor circuit | (see page 21-141)

In case of multiple problems, the recirculation indicator light will indicate only the DTC with the least number of blinks.