## Seats

#### Rear Seat-back Cover Replacement – Folding Type (cont'd)

20-100

5. If equipped with a headrest, pull out the seat-back frame (A) from the pad (B), then pull out the headrest guides (C) while pinching the end of the guides, and remove them. The left seat-back is shown, the right seat-back is similar.

6. Remove the seat-back cover and pad from the seat-back frame.

7. Pull back the edge of the seat-back cover (A) all the way around, and release the hooks (B) of the horizontal wires (C) from the vertical wires (D) on the pad, and on the left seat-back, remove the clips (E), then remove the seat-back cover.

Left seat-back:

Right seat-back:

8. Install the cover in the reverse order of removal, and note these items:

- To prevent wrinkles when installing a seat-back cover, make sure the material is stretched evenly over the pad before securing the hooks and clips.
- Replace any clips you removed with new ones. Install them with commercially available upholstery ring pliers.