## Climate Control

#### Outside Air Temperature Sensor Replacement (cont'd)

21-151
Outside Air Temperature Sensor Test

5-door

1. Release the lock and remove the outside air temperature sensor, then disconnect the 2P connector.

2. Install the sensor in the reverse order of removal.

Dip the sensor in ice water and measure the resistance. Then pour hot water on the sensor and check for a change in resistance.

Compare the resistance reading between the No. 1 and No. 2 terminals of the outside air temperature sensor with the specifications shown in the graph; the resistance should be within the specifications.