## Honda Multi Matic Transmission/CVT

#### Shift Cable Replacement

14-343

1. Raise the vehicle and make sure it is securely supported (see page 1-15).

2. Shift the transmission into position.
3. Remove the centre console panel and centre console (see page 20-73).
4. Remove the nut securing the shift cable end (A), then separate the cable end from the shift lever assembly.

5. Rotate the socket holder (A) on the shift cable (B) toward the shift lever a quarter turn, then slide the holder out to remove the shift cable from the shift cable bracket base (C).

   NOTE: Do not remove the shift cable by twisting the shift cable guide (D).

6. Disconnect the secondary HO2S connector and remove the exhaust pipe A and the heat shield (B).

7. Remove the shift cable guide brackets (A) and grommet (B).