## Engine Assembly

#### Engine Installation (cont'd)

5-12

1. Tighten the rear mount mounting bolts.

1. Lower the hoist.

1. Tighten the upper bracket mounting bolt and nut.

1. Tighten the support bolt and nuts.

1. Remove the chain hoist from the engine.

1. Raise the hoist to full height.

1. Install a new spring clip on the end of each driveshaft, then install the driveshafts. Make sure each clip ''clicks'' into place in the differential and intermediate shaft.

1. Connect the suspension lower arm ball joints (see step 10 on page 18-5) and stabiliser links (see step 9 on page 18-5).

a a a