## Automatic Transmission

#### Shift Cable Adjustment

14-151

4-door Model

1. Shift the transmission into position.
2. Remove the centre console panel and centre console (see page 20-73).
3. Remove the nut securing the shift cable end (A), then separate the cable end from the shift lever assembly.

4. Rotate the socket holder (A) on the shift cable (B) toward the shift lever a quarter turn, then slide the holder out to remove the shift cable from the shift cable bracket base (C).

NOTE: Do not remove the shift cable by twisting the shift cable guide (D).

5. Push the shift cable until it stops, then release it. Pull the shift cable back 2 steps so that the shift position is in

6. Turn the ignition switch ON (II) and verify that the position indicator light comes on.
7. Turn the ignition switch OFF.
8. Insert a 6.0 mm (0.24 in.) pin (A) through the positioning hole (B) on the shift lever bracket base and into the positioning hole (C) on the shift lever assembly.