## Manual Transmission

#### Transmission Removal (cont'd)

13-5

8. Remove the starter motor.

9. First remove the cable bracket (A), then disconnect the cables (B) from the top of the transmission housing. Carefully remove both cables and the bracket together so as not to bend the cables.

10. Disconnect the vehicle speed sensor (VSS) connector.

11. Attach the chain hoist (A) to the engine using the 8 x 1.25 mm bolt (B).