## Standards and Service Limits

#### Steering

2-6

Item | Measurement | Qualification | Standard or New | Service Limit
Steering wheel | Rotational play measured at outside edge | With engine running | 0 – 10 mm (0 – 0.39 in.) | –
Starting load measured at outside edge | With engine running | 29 N (3.0 kgf, 6.6 lbs) | –
Gearbox | Angle of rack guide screw loosened from locked position |  | 5° Max.

Suspension

Item | Measurement | Qualification | Standard or New | Service Limit
Wheel alignment | Camber | Front | 0°00'+45°
Rear | –0°45'+45'
Caster | Front | 1°33'+1°
Total Toe | Front | 0+3 mm (0+0.12 in.)
Rear | Adjust: IN 2 +2/-1mm (0.08 +0.08/-0.04 in.) Inspect: IN 2 + 3 mm (0.08+0.12 in.)
Front wheel turning angle | Inside wheel | 40°00'+2°
Outside wheel | 31°00' (Reference)
Aluminium wheel | Runout | Axial | 0 – 0.7 mm (0 – 0.03 in.) | 2.0 mm (0.08 in.)
Radial | 0 – 0.7 mm (0 – 0.03 in.) | 1.5 mm (0.06 in.)
Steel wheel | Runout | Axial | 0 – 1.0 mm (0 – 0.04 in.) | 2.0 mm (0.08 in.)
Radial | 0 – 1.0 mm (0 – 0.04 in.) | 1.5 mm (0.06 in.)
Wheel bearings | End play | Front | 0 – 0.05 mm (0 – 0.002 in.)
Rear | 0 – 0.05 mm (0 – 0.002 in.)

a a a