## Engine Block

#### Crankshaft Installation (cont'd)

7-20

Oil Pan Installation

1. Apply a bead (A) of liquid gasket to sealing surfaces of crankshaft seal ring retainer (B).

1. Install crankshaft seal retainer to rear of cylinder block.

Specified torque:

9.8 Nm (1.0 kgf/m, 7.2 lbf/ft)

NOTE: Recut thread before re-use and insert bolts with screw locking compound. The installation time including the torque check is max. 10 min.

1. Apply engine oil to oil seal lip.

1. Install oil seal to oil seal retainer using special tool (5-8840-7005-0; without crankshaft or 5-8840-7006-0; with crankshaft).

Special Tool Required

Aligner 5-8840-9054-0

1. Clean the sealing surfaces of the upper oil pan and remove the sealant residue.

1. Apply a bead of liquid gasket to sealing surfaces on the oil pan upper.

1. Install aligner (special tool) (A) (5-8840-9054-0) to oil pan upper with tightening torque 9.8 Nm (1.0 kgf/m, 7.2 lbf/ft).

a a a