## Clutch

#### Clutch Master Cylinder Overhaul

12-7

Exploded View

1. Clip catches shall be on arrow marked side
2. RESERVIOUR HOSE

   Inspect for damage, leaks, interference and twisting

3. CLUTCH LINE CONNECTOR
4. O-RING

   Replace.

5. RESERVIOR
6. RETAINING CLIP

   Replace.

7. MASTER CYLINDER BODY

   Check the cylinder wall for scoring and wear.

8. (Brake Assembly Lube)
9. PUSH ROD
10. CIRCLIP
11. LOCK PIN

    Replace.

12. YOKE
13. PEDAL PIN
14. STOPPER

    Check for damage and bending

15. CLUTCH MASTER CYLINDER SEAL
16. O-RING

    Replace.

17. CONNECTOR

a a a