## ABS Components

#### System Description (cont'd)

19-63

Terminal number | Wire colour | Terminal sign (Terminal name) | Description | Measurement
Terminals | Conditions (Ignition switch ON (II)) | Voltage
14 | WHT/BLK | STOP | Detects brake switch signal | 14-GND | Brake pedal | Pressed | Battery voltage
Released | 0 V
15 | BLK/ORN | IG2 | Power source for activating the system | 15-GND | ——— | Battery voltage
16 | BLK | M – GND (Motor ground) | Ground for the pump motor | 16-GND | ——— | Below 0.3 V
17 | WHT/RED | + B – MR (+ B motor relay) | Power source for the pump motor | 17-GND | At all times | Battery voltage
18 | WHT/GRN | +B-FSR (+B fail-safe relay) | Power source for the valve relay | 18-GND | At all times | Battery voltage
19 | BLK | GND | Ground for the modulator assembly | 19-GND | ——— | Below 0.3 V
20 | BLU/RED | ABS | Drives ABS indicator | 20-GND | ABS indicator | ON | About 11 V
OFF | Below 1 V
21 | BRN/YEL | EBD (Electronic brake distribution) | Drives brake system indicator | 21-GND | Engine running, parking brake | Pulled | Below 0.3 V
Released | Battery voltage