## Power Distribution

#### Fuse to Components Index (cont'd)

22-7

Under-dash Fuse/Relay Box

Fuse Number | Amps | Wire Colour | Component(s) or Circuit(s) Protected
1 | 15 A | BLK/WHT | Ignition coils
2 | - | - | Not used
3 | 10 A | RED/BLU | Multiplex control unit
4 | 10 A | BLK/ORN | Alternator, Cruise control unit, Evaporative emission (EVAP) canister purge valve, Primary and secondary HO2S, Vehicle speed sensor (VSS)
5 | 7.5 A | Fuse/relay box socket | Multiplex control unit (KG)
6 | 7.5 A | YEL/GRN | Sunroof open and close relays, Power window relay, Headlight adjuster unit
7 | 20 A | GRN | Sunroof motor
8 | 7.5 A | YEL/RED | Audio unit, Multiplex control unit
9 | 10 A | GRN | OPDS unit
10 | 7.5 A | YEL | A/T reverse relay, Back-up lights, Gauge assembly, Keyless receiver unit, Multiplex control unit, Security control unit, Shift lock solenoid
11 | 7.5 A | BLK/ORN | ABS modulator-control unit (IG2)
12 | 7.5 A | YEL/RED | Multiplex control unit (KG)
13 | 10 A | PNK | SRS unit
14 | 10 A | BLK/YEL | A/C compressor fan relay, Heater control panel/climate control unit, Condenser fan relay, Blower motor relay, Power mirror actuators, Radiator fan relay, Recirculation control motor, Rear window defogger relay
15 | 30 A | RED/YEL | Headlight washer control unit (KG, KR)
16 | 20 A | RED/BLK | Seat heaters
17 | 15 A | BLK/YEL | ECM/PCM, SRS unit
18 | 15 A | YEL/GRN | Cigarette lighter
19 | 7.5 A | YEL/BLK | Turn signal/hazard relay
20 | 20 A | GRN/BLK | Multiplex control unit, Windshield washer motor, Windshield wiper motor
21 | - | - | Not used
22 | 20 A | GRN/BLK | Passenger's power window motor
23 | 20 A | GRN/WHT | Driver's power window motor