## Engine Assembly

#### Engine Installation (cont'd)

5-11

1. Position the engine under the vehicle. Attach the chain hoist to the engine, then lift the engine into position in the vehicle.

Reinstall the mounting bolts/support nuts in the sequence given. Failure to follow this sequence may cause excessive noise and vibration, and reduce bushing life.

1. Install the A/C compressor (A), and connect the compressor clutch connector (B).

1. Install the sub-frame (A). Align the reference lines (B) on the sub-frame with the bolt head centre, then tighten the bolts.

1. Tighten the front mount mounting bolt.

a a a