## Manual Transmission

#### Countershaft Assembly Clearance Inspection (cont'd)

13-31

3. Measure the clearance between the 2nd gear (A) and 3rd gear (B) with a feeler gauge (C). If the clearance is more than the service limit, go to step 4.

Standard: | 0.04 - 0.12 mm (0.002 - 0.005 in.)
Service Limit: | 0.24 mm (0.009 in.)

4. Measure the thickness of the spacer collar.

- If the thickness is less than the service limit, replace the spacer collar with a new one.
- If the thickness is within the service limit, go to step 5.

Standard: | 27.53 - 27.56 mm (1.084 - 1.085 in.)
Service Limit: | 27.51 mm (1.083 in.)

5. Measure the thickness of 2nd gear.

- If the thickness of 2nd gear is less than the service limit, replace 2nd gear with a new one.
- If the thickness of 2nd gear is within the service limit, replace the 1st/2nd synchro hub with a new one.

Standard: | 27.41 – 27.46 mm (1.079 – 1.081 in.)
Service Limit: | 27.36 mm (1.077 in.)