## PGM-FI System

#### DTC Troubleshooting (cont'd)

11-393

DTC P1107: BARO Sensor Circuit Low Voltage

DTC P1108: | BARO Sensor Circuit High Voltage

1. Reset the ECM/PCM (see page 11-312).
2. Turn the ignition switch ON (II).

Is DTC P1107 or P1108 indicated?

YES | - Substitute a known-good ECM/PCM and recheck (see page 11-313). If symptom/indication goes away, replace the original ECM/PCM.
NO | - Intermittent failure, system is OK at this time.