## SRS

#### DTC Troubleshooting (cont'd)

23-91

DTC 9-7: Faulty Right Front Sensor

1. Erase the DTC memory (see page 23-38).
2. Turn the ignition switch ON (II), and check that the SRS indicator light comes on for about 6 seconds and then goes off.

Does the SRS indicator light stay on?

YES - Go to step 3.

NO - Intermittent failure, system is OK at this time. Go to Troubleshooting Intermittent Failures (see page 23-38).

3. Turn the ignition switch OFF. Check the connections between the dashboard wire harness B 18P connector and the SRS unit, and between the engine compartment wire harness 2P connector and the right front sensor for 4-door model (see page 23-23) or 5-door model (see page 23-24).

Are the connections OK?

YES - Go to step 4.

NO - Poor contact at the SRS unit and/or right front sensor; reconnect or replace them.

4. Disconnect the battery negative cable and wait for 3 minutes.
5. Disconnect the D1o connector from the D1i connector (A).

6. Disconnect the P1o connector from the P1i connector (A).

7. Disconnect the TL1o and TR1o connectors from the TL1i and TR1i connectors (A).